                   

[image: ]SPECIFICATIONS – SC 800 (WIND-RESISTANT SCREEN)  
Harol or equivalent
The sun blind is fitted in front of or on the window frame. The fabric is tightly attached to the guide rails to prevent it from being blown out by the wind.
Wind speed class                                                                                                                                                                                       These comply with wind speed class 3 – EN13561. Test results according to CSTC, running at constant pressure of up to 1000Pa (up to >140km/h) and an average dimension of 3.5 x 3m.
Box                                                                                                                                                                                               The box (square or rounded) is made of extruded aluminium, which is powder-coated (colour to be chosen by the architect) 
The box dimensions are 73 x 73, 90 x 90, 110 x 110, 150 x 150mm (based on the rolled-up size of the fabric).
The box consists of a square or rounded front plate, a torque bar and an upper plate. The upper plate has guide rail grooves for mounting brackets that can be fitted optionally. The screen is assembled with stainless steel screws. The metal side cap has a guide pin and stop to fit the guide rail into.
Fabric
a) Serge 
This is a transparent and light-inhibitory fabric consisting of fibre-optic threads which are pre-coated with plastic-based PVC and mass-coloured. The fabric retains its shape, is not affected by moisture and heat, unperishable and resistant to light. The vertical lateral sections of the fabric are reinforced by a high-frequency zip (on the non-visible side).  The bottom is strengthened by an applied reinforcement band. The darkest side is positioned on the outside or view side. For heights of more than 2,500 mm, there is a horizontal weld seam.
· Weight per m²: approx. 525 gr/m² 
· Thickness: 0.84 mm
· Classification of flammability: M1
· Colour: to be determined by the architect in charge




b) Soltis 86 / Soltis 92
These are transparent and light-inhibiting fabrics, consisting of woven polyester threads which are stretched under great tension and attached with a Plastisol layer.  The fabrics have a two-sided coating, giving the fabrics excellent protection against UV rays and making them dirt-repellent.  The vertical lateral sections of the fabric are reinforced by a high-frequency zip (on the non-visible side).  The bottom is strengthened by an applied reinforcement band.  For heights of more than 1.770 mm, there is a horizontal weld seam!
· Weight per m²: approx. 380-420 gr/m² 
· Thickness: 0.43-0.45 mm
· Classification of flammability: /M1/B1
· Colour: to be determined by the architect in charge

c) Black-out B92 
This is a transparent and light-inhibiting fabric, consisting of woven polyester threads which are stretched under great tension and attached with a Plastisol layer (Soltis).  On the window side of the fabric, an obscuring PVC coating has been applied.  The vertical lateral sections of the fabric are reinforced by a high-frequency welded zip (on the Soltis side).  The bottom is strengthened by an applied reinforcement band. For heights of more than 1700 mm, there is a horizontal weld seam.
· Weight per m²: approx. 650 gr/m² 
· Thickness: 0.60 mm
· Classification of flammability: M2
· Colour: to be determined by the architect in charge

Control system
Manual: Crank handle operation:										 - self-braking worm-worm gear mechanism, with a transmission capacity of 1:4, a built-in end limiter (prevents the fabric from rolling up incorrectly)
Electric: Operation consists of a built-in, asynchronous tubular motor with adjustment buttons for determining the up and down position.
Optional extras:
· Motors with electronic shut-off.
· Motors with built-in receiver (RTS)
· Control, by room and centrally by wind-sun sensing device.
To be carried out by electrician: cables for power supply and operation of the sun protection screens.
Guide rails											     Clip guides with blind attachment from extruded aluminium, with a powder coating or natural-coloured anodised. At the bottom there is an end cap to stop the bottom lath.
External dimensions 55 x 30mm or 40 x 30
Inside the guide rail there is a plastic strip with metal springs which keeps the fabric tight.
Bottom lath and sliding block										        The bottom lath is made of extruded aluminium, which is powder-coated (colour to be chosen by the architect). The weight of the bottom lath (including the strengthening strip) is 1.6 kg per metre.
Fabric is attached to bottom lath without screws, using a plastic tube. 
Fabric roll												        The fabric roll is made from extruded aluminium.
- It has a groove for attaching the fabric with
  a fabric rod with a diameter of 3 or 4 mm.
- Various types of fabric rolls are available, depending on type of operation,
  quality of the fabric, and box type:
Electric operation:  spindle Ø 55 mm, Ø 67 mm of steel straps spindle Ø 85mm.
For manual control also spindle Ø 40mm

Multiple screens 
Ability to use 1 box for 2 or 3 screens: 
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· type 1: screens directly next to each other (DVC)
type 2: screens with a small gap (DVS):
· minimum 26 mm
maximum 500 mm
Available with 1 or 2 operation systems:
- Maximum overall width per operation:
- Electric operation can be coupled up to 6 m.
	- Operating unit can never be placed at the coupling side of the fabric roll;
	- Likewise it is recommended to place the operating unit next to the largest screen when possible.
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